|  |  |  |  |
| --- | --- | --- | --- |
| small APTlogogreen | ASIA-PACIFIC TELECOMMUNITY |  |  |
| **The APT Conference Preparatory Group for WRC-15**  |  |
|  |  |

Source: APG15-3/OUT-13

**preliminary views on WRC-15 agenda item 1.7**

**Agenda Item 1.7:** *to review the use of the band 5 091-5 150 MHz by the fixed-satellite service (Earth‑to‑space) (limited to feeder links of the non-geostationary mobile-satellite systems in the mobile-satellite service) in accordance with Resolution****114 (Rev.WRC‑12)***

Resolution **114 (Rev.WRC-12)**: *Studies on compatibility between new systems of the aeronautical radionavigation service and the fixed‑satellite service (Earth-to-space) (limited to feeder links of the non‑geostationary mobile-satellite systems in the mobile-satellite service) in the frequency band 5 091‑5 150 MHz*

**APT Preliminary Views:**

APT Members support the current Method A of the draft CPM text as shown in Annex 23 of Document 4A/468. APT Members also noted that the future application of ARNS systems in the band 5091-5150MHz should be protected from harmful interference and the development should not be limited.

\_\_\_\_\_\_\_\_\_\_\_\_